<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="MD0707029CE.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE9">9 Self Diagnosis and Special Mode Setting</html:a>
</ttl>
<p>This unit is equipped with functions for checking and inspecting.
</p>
<ti2 module="0">
<ttl><html:a name="TITLE9_1">9.1 Service Mode Summary Table</html:a>
</ttl>
<ti3 module="0">
<ttl><html:a name="TITLE9_1_1">9.1.1 Service Mode Summary Table (For DVD)</html:a>
</ttl>
<p>The service modes can be activated by pressing various button combination on the main unit and remote control unit.
</p>
<p>Below is the summary for the various modes for checking: 
</p>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="4" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="1.110in">
</colspec>
<colspec colnum="2" colname="2" colwidth="1.573in">
</colspec>
<colspec colnum="3" colname="3" colwidth="3.202in">
</colspec>
<colspec colnum="4" colname="4" colwidth="1.311in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Main buttons
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Remote control unit buttons
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Application
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Note
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="17" align="center"><html:td valign="top" align="center" colspan="1" rowspan="18">
<p>[STOP]
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[0]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Error code display.
</p>
</html:td></entry>
<entry colname="4" morerows="2" align="left"><html:td valign="top" align="left" colspan="1" rowspan="3">
<p>(Refer to the section &#8220;9.2.1. 
<xref rid="cihdaafh" type="txt"><html:a href="MD0707029CE_09.xml#cihdaafh">Service Mode Table 1</html:a>
</xref>&#8221; for more information.)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[5]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Jitter checking.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[PAUSE]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initial setting of laser drive current.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[FUNCTIONS]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DVD laser drive current check.
</p>
</html:td></entry>
<entry colname="4" morerows="2" align="left"><html:td valign="top" align="left" colspan="1" rowspan="3">
<p>(Refer to the section &#8220;9.2.2. 
<xref rid="cihdfcgf" type="txt"><html:a href="MD0707029CE_09.xml#cihdfcgf">Service Mode Table 2</html:a>
</xref>&#8221; for more information.)
</p>
<p>
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[1]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ADSC internal RAM data check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[3]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>CD laser drive current check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[6]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Region display and mode.
</p>
</html:td></entry>
<entry colname="4" morerows="2" align="left"><html:td valign="top" align="left" colspan="1" rowspan="3">
<p>(Refer to the section &#8220;9.2.3. 
<xref rid="cihgcghf" type="txt"><html:a href="MD0707029CE_09.xml#cihgcghf">Service Mode Table 3</html:a>
</xref>&#8220; for more information.)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[7]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Micro-processor firmware version check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic27" sizex="9.991mm" sizey="7.366mm"><html:img src="v9rem_10.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initialization of the player (factory setting is restored).
</p>
<p>Used after replacement of Micro-processor (DV5 LSI) IC, FLASH ROM IC (IC8651), EEPROM IC (IC8611) and DVD Module P.C.B.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[8]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DVD Module P.C.B. firmware version check.
</p>
</html:td></entry>
<entry colname="4" morerows="4" align="left"><html:td valign="top" align="left" colspan="1" rowspan="5">
<p>(Refer to the section &#8220;9.2.4. 
<xref rid="cihhjifd" type="txt"><html:a href="MD0707029CE_09.xml#cihhjifd">Service Mode Table 4</html:a>
</xref>&#8220; for more information.)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[MENU]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Communication error display.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[TOP MENU]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ECC error check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[DISC]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>CPPM&#47;CRM keys check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[ENTER]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DVD Module P.C.B. reset.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic28" sizex="6.519mm" sizey="6.181mm"><html:img src="v9up.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer 1 check.
</p>
</html:td></entry>
<entry colname="4" morerows="3" align="left"><html:td valign="top" align="left" colspan="1" rowspan="4">
<p>(Refer to the section &#8220;9.2.5. 
<xref rid="cihfeiia" type="txt"><html:a href="MD0707029CE_09.xml#cihfeiia">Service Mode Table 5</html:a>
</xref>&#8220; for more information.)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic29" sizex="6.519mm" sizey="6.181mm"><html:img src="v9down.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer 1 reset.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic30" sizex="6.181mm" sizey="6.519mm"><html:img src="v9right.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer 2 check.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic31" sizex="6.181mm" sizey="6.519mm"><html:img src="v9left.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer 2 reset.
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<p>
</p>
<caution>
<ttl>Note:
</ttl>
<p>An error code will be canceled if a power supply is turned OFF.
</p>
<p>&#42;1: CPPM is the copy guard function beforehand written in the disk for protection of copyrights.
</p>
<p>&#42;2: CEC is the consumer electronic control used for high-level user control of HDMI-connected devices.
</p>
<p>&#42;3: HDCP is the specification developed to control digital audio &#38; video contents transmission for DVI or HDMI connections.
</p>
</caution>
<p>
</p>
<p>
</p>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_1_2">9.1.2 Service Mode Summary Table (For Inspection)</html:a>
</ttl>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="4" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="1.110in">
</colspec>
<colspec colnum="2" colname="2" colwidth="1.573in">
</colspec>
<colspec colnum="3" colname="3" colwidth="3.202in">
</colspec>
<colspec colnum="4" colname="4" colwidth="1.311in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Main buttons
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Remote control unit buttons
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Application
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Note
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[STOP] &#43;
</p>
<p>[
<graphic loc="graphic32" sizex="7.112mm" sizey="6.689mm"><html:img src="v9tup.png" border="0"></html:img>
</graphic>&#47;FF&#47;
<graphic loc="graphic33" sizex="9.567mm" sizey="6.181mm"><html:img src="v9fskip.png" border="0"></html:img>
</graphic>]
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>-
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Entering self-diagnostic mode.
</p>
</html:td></entry>
<entry colname="4" morerows="3" align="left"><html:td valign="top" align="left" colspan="1" rowspan="4">
<p>(Refer to the section &#8220;9.3.1. 
<xref rid="chdedbdh" type="txt"><html:a href="MD0707029CE_09.xml#chdedbdh">Service Mode Table 1</html:a>
</xref>&#8221; for more information.)
</p>
<p>
</p>
<p>
</p>
<p>
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="2">
<p>In Self-diagnostic Mode
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p> [1]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DVD&#47;CD Changer Mechanism Reliability Test.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p> [SINGLE CHANGE]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Servicing the traverse unit.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[STOP]
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[4] &#43; [7]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Entering doctor mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="5">
<p>In Doctor Mode
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[STOP] button on the main unit &#43; [4] &#43; [7]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Firmware version check.
</p>
</html:td></entry>
<entry colname="4" morerows="3" align="left"><html:td valign="top" align="left" colspan="1" rowspan="4">
<p>(Refer to the section &#8220;9.3.2. 
<xref rid="chdcifje" type="txt"><html:a href="MD0707029CE_09.xml#chdcifje">Service Mode Table 2</html:a>
</xref>&#8220; for more information.)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[4]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Cold start.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[0]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Tape eject test.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[
<graphic loc="graphic34" sizex="7.535mm" sizey="7.535mm"><html:img src="v9timer.png" border="0"></html:img>
</graphic>PLAY&#47;REC]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>FL display test.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>[DISC]
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DVD&#47;CD changer operation check.
</p>
</html:td></entry>
<entry colname="4" align="left"><html:td valign="top" align="left" colspan="1" rowspan="1">
<p>(Refer to the section &#8220;9.3.3. 
<xref rid="beibijjh" type="txt"><html:a href="MD0707029CE_09.xml#beibijjh">Service Mode Table 3</html:a>
</xref>&#8220; for more information.)
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<p>
</p>
<p>
</p>
</ti3>
</ti2>
<ti2>
<ttl><html:a name="TITLE9_2">9.2 Service Mode Table (For DVD)</html:a>
</ttl>
<p>By pressing various button combinations on the player and remote control unit can activate the various service modes for checking.
</p>
<topic>
<ttl>Special Note:
</ttl>
<p>Due to the limitations of the no. characters that can be shown on FL Display, the &#8220;FL Display&#8221; button on the remote control unit is used to show the following page. (Display 1 &#47; Display 2).
</p>
</topic>
<ti3 module="0">
<ttl id="cihdaafh"><html:a name="TITLE9_2_1"><html:a name="cihdaafh">9.2.1 Service Mode Table 1</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic35" sizex="180.000mm" sizey="219.054mm"><html:center><html:a href="v9smtm1.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="cihdfcgf"><html:a name="TITLE9_2_2"><html:a name="cihdfcgf">9.2.2 Service Mode Table 2</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic36" sizex="180.000mm" sizey="207.708mm"><html:center><html:a href="v9smtm2.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="cihgcghf"><html:a name="TITLE9_2_3"><html:a name="cihgcghf">9.2.3 Service Mode Table 3</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic37" sizex="180.000mm" sizey="223.397mm"><html:center><html:a href="v9smtm3.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
<fig type="ext">
<cap>Fig. 9.1
</cap>
<graphic loc="graphic38" sizex="180.000mm" sizey="240.000mm"><html:center><html:a href="v9vdi.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="cihhjifd"><html:a name="TITLE9_2_4"><html:a name="cihhjifd">9.2.4 Service Mode Table 4</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic39" sizex="180.000mm" sizey="198.703mm"><html:center><html:a href="v9smtm4.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="cihfeiia"><html:a name="TITLE9_2_5"><html:a name="cihfeiia">9.2.5 Service Mode Table 5</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic40" sizex="180.000mm" sizey="176.654mm"><html:center><html:a href="v9smtm5.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_2_6">9.2.6 Optical Pickup Unit Breakdown Diagnosis </html:a>
</ttl>
<p>The unit is equipped with the optical pickup self-diagnosis function and tilt adjustment check function. Follow the procedure described below during repair in order to perform self-diagnosis and tilt adjustment effectively. Especially when "NO DISC"
is displayed, be sure to apply the self-diagnosis function before replacing with an optical pickup. Replacement of optical pickup generally requires when the present value of laser drive exceeds 23 (DVD) or 34 (CD).</p>
<topic>
<ttl>Note:
</ttl>
<p>Start diagnosis within three minutes after tuning on the power (as diagnosis fails when the unit becomes warm).
</p>
</topic>
<fig type="ext">
<graphic loc="graphic41" sizex="158.750mm" sizey="179.917mm"><html:center><html:a href="v9opsd.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
</ti2>
<ti2>
<ttl><html:a name="TITLE9_3">9.3 Service Mode Table (For Inspection)</html:a>
</ttl>
<ti3 module="0">
<ttl id="chdedbdh"><html:a name="TITLE9_3_1"><html:a name="chdedbdh">9.3.1 Service Mode Table 1</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic42" sizex="180.000mm" sizey="204.523mm"><html:center><html:a href="v9spmt1.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="chdcifje"><html:a name="TITLE9_3_2"><html:a name="chdcifje">9.3.2 Service Mode Table 2</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic43" sizex="180.000mm" sizey="222.251mm"><html:center><html:a href="v9spmt2.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl id="beibijjh"><html:a name="TITLE9_3_3"><html:a name="beibijjh">9.3.3 Service Mode Table 3</html:a></html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic44" sizex="180.000mm" sizey="132.777mm"><html:center><html:a href="v9spmt3.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
<p>
</p>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_3_4">9.3.4 CD&#47;DVD changer unit ageing test mode</html:a>
</ttl>
<p>Below is the process flow chart of ageing for the CD&#47;DVD changer unit. (CRS1D)
</p>
<fig type="ext">
<graphic loc="graphic45" sizex="129.470mm" sizey="240.000mm"><html:center><html:a href="v9mode1.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
<fig type="ext">
<graphic loc="graphic46" sizex="129.470mm" sizey="140.500mm"><html:center><html:a href="v9mode2.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
</ti2>
<ti2>
<ttl id="babfegbh"><html:a name="TITLE9_4"><html:a name="babfegbh">9.4 DVD Self Diagnostic Function-Error Code</html:a></html:a>
</ttl>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_1">9.4.1 DVD Module Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic47" sizex="180.000mm" sizey="240.000mm"><html:center><html:a href="v9hmect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_2">9.4.2 Mechanism Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic48" sizex="180.000mm" sizey="240.000mm"><html:center><html:a href="v9mect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_3">9.4.3 Power Supply Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic49" sizex="180.000mm" sizey="88.503mm"><html:center><html:a href="v9psect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_4">9.4.4 ECC Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic50" sizex="180.000mm" sizey="79.111mm"><html:center><html:a href="v9eect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_5">9.4.5 USB Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic51" sizex="180.000mm" sizey="101.644mm"><html:center><html:a href="v9uect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_6">9.4.6 CD&#47;DVD Changer Mechanism Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic52" sizex="180.000mm" sizey="240.000mm"><html:center><html:a href="v9cmect1.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
<fig type="ext">
<graphic loc="graphic53" sizex="180.000mm" sizey="178.771mm"><html:center><html:a href="v9cmect2.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_4_7">9.4.7 Deck Mechanism Error Code Table</html:a>
</ttl>
<fig type="ext">
<graphic loc="graphic54" sizex="180.000mm" sizey="240.000mm"><html:center><html:a href="v9dmect.pdf" target="_self"><html:img src="pana.gif" border="0"></html:img></html:a></html:center>
</graphic>
</fig>
</ti3>
</ti2>
<ti2>
<ttl><html:a name="TITLE9_5">9.5 Sales Demonstration Lock Function</html:a>
</ttl>
<p>This function prevents discs from being lost when the unit is used for sales demonstrations by disabling the disc eject function.  "LOCKED" is displayed on the unit, and ordinary operation is disabled.
</p>
<ti3 module="0">
<ttl><html:a name="TITLE9_5_1">9.5.1 Setting</html:a>
</ttl>
<ul>
<li>
<p>
<emp>Prohibiting removal of disc
</emp>
</p>
<ol>
<li>
<p>Select &#8220;DVD&#47;CD&#8221; mode.
</p>
</li>
<li>
<p>At POWER ON condition, press and hold down the STOP
<graphic loc="graphic55" sizex="6.265mm" sizey="6.265mm"><html:img src="v9stop.png" border="0"></html:img>
</graphic>button and the AC IN
<graphic loc="graphic56" sizex="8.213mm" sizey="6.773mm"><html:img src="v9stndby.png" border="0"></html:img>
</graphic>button on the main unit for at least three seconds.
(The message, &#8220;___LOCKED_&#8221; appears when the function is activated.)</p>
</li>
</ol>
<topic>
<ttl>Note:
</ttl>
<p>OPEN&#47;CLOSE
<graphic loc="graphic57" sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, MULTI CHANGE
<graphic loc="graphic57" sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, SINGLE CHANGE
<graphic loc="graphic57" sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, TAPE
<graphic    loc="graphic58" sizex="8.975mm" sizey="6.435mm"><html:img src="v9tape.png" border="0"></html:img>
</graphic>, TUNER&#47;BAND, EXT-IN, RECORD
<graphic loc="graphic59" sizex="6.435mm" sizey="6.350mm"><html:img src="v9record.png" border="0"></html:img>
</graphic> is invalid and the main unit displays &#8220;___LOCKED_&#8221; while the lock function
mode is entered.</p>
</topic>
<p>
</p>
</li>
<li>
<p>
<emp>Prohibiting operation of selector and disc
</emp>
</p>
<ol>
<li>
<p>Select the &#8220;DVD&#47;CD&#8221; mode.
</p>
</li>
<li>
<p>At POWER ON condition, press and hold down the DVD&#47;CD
<graphic loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>button and the AC IN
<graphic loc="graphic56" sizex="8.213mm" sizey="6.773mm"><html:img src="v9stndby.png" border="0"></html:img>
</graphic>button on the main unit for at least
three seconds. (The message, &#8220;___LOCKED_&#8221; appears when the function is activated.)</p>
</li>
</ol>
<topic>
<ttl>Note:
</ttl>
<p>The following buttons are invalid and the main unit displays  &#8220;___LOCKED_&#8221;  while the lock function mode is entered.
</p>
</topic>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="2" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.787in">
</colspec>
<colspec colnum="2" colname="2" colwidth="5.905in">
</colspec>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Main unit
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>OPEN&#47;CLOSE
<graphic loc="graphic57" sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, MULTI CHANGE
<graphic loc="graphic57" sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, SINGLE CHANGE
<graphic loc="graphic57"    sizex="6.435mm" sizey="6.519mm"><html:img src="v9eject.png" border="0"></html:img>
</graphic>, 1
<graphic loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>, 2
<graphic loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>, 3
<graphic loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>, 4
<graphic    loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>, 5
<graphic loc="graphic60" sizex="6.265mm" sizey="6.265mm"><html:img src="v9play.png" border="0"></html:img>
</graphic>, STOP
<graphic loc="graphic55" sizex="6.265mm" sizey="6.265mm"><html:img src="v9stop.png" border="0"></html:img>
</graphic>, 
<graphic loc="graphic32" sizex="7.112mm"    sizey="6.689mm"><html:img src="v9tup.png" border="0"></html:img>
</graphic>&#47;FF
<graphic loc="graphic33" sizex="9.567mm" sizey="6.181mm"><html:img src="v9fskip.png" border="0"></html:img>
</graphic>, 
<graphic loc="graphic61" sizex="7.112mm" sizey="6.689mm"><html:img src="v9tdown.png" border="0"></html:img>
</graphic>&#47;REW
<graphic loc="graphic62" sizex="9.567mm" sizey="6.181mm"><html:img src="v9rskip.png" border="0"></html:img>
</graphic>, TAPE
<graphic    loc="graphic58" sizex="8.975mm" sizey="6.435mm"><html:img src="v9tape.png" border="0"></html:img>
</graphic>, TUNER&#47;BAND, EXT-IN, RECORD
<graphic loc="graphic59" sizex="6.435mm" sizey="6.350mm"><html:img src="v9record.png" border="0"></html:img>
</graphic> 
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p> Remote controller unit
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>NUMERIC KEYS 0~9, 
<graphic loc="graphic27" sizex="9.991mm" sizey="7.366mm"><html:img src="v9rem_10.png" border="0"></html:img>
</graphic>, 
<graphic loc="graphic55" sizex="6.265mm" sizey="6.265mm"><html:img src="v9stop.png" border="0"></html:img>
</graphic>, 
<graphic loc="graphic63" sizex="6.011mm" sizey="6.096mm"><html:img src="v9pause.png" border="0"></html:img>
</graphic>, 
<graphic    loc="graphic32" sizex="7.112mm" sizey="6.689mm"><html:img src="v9tup.png" border="0"></html:img>
</graphic>&#47;FF
<graphic loc="graphic33" sizex="9.567mm" sizey="6.181mm"><html:img src="v9fskip.png" border="0"></html:img>
</graphic>, 
<graphic loc="graphic61" sizex="7.112mm" sizey="6.689mm"><html:img src="v9tdown.png" border="0"></html:img>
</graphic>&#47;REW
<graphic loc="graphic62" sizex="9.567mm"    sizey="6.181mm"><html:img src="v9rskip.png" border="0"></html:img>
</graphic>, SLOW&#47;SEARCH
<graphic loc="graphic64" sizex="9.313mm" sizey="6.181mm"><html:img src="v9rsrch.png" border="0"></html:img>
</graphic>&#47;
<graphic loc="graphic65" sizex="9.313mm" sizey="6.181mm"><html:img src="v9fsrch.png" border="0"></html:img>
</graphic>, FUNCTIONS, RETURN&#47;SETUP, FL DISPLAY, MUTING&#47;CANCEL,
MENU&#47;PLAY LIST, CH SELECT&#47;TEST, EXT-IN, TUNER&#47;BAND, CLOCK&#47;TIMER, SLEEP&#47;A. OFF, DISC, TAPE<graphic loc="graphic58" sizex="8.975mm" sizey="6.435mm"><html:img src="v9tape.png" border="0"></html:img>
</graphic>, REPEAT, AUDIO.
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</li>
</ul>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE9_5_2">9.5.2 Cancellation</html:a>
</ttl>
<p>The lock can be cancelled by the same procedure as used in setting. ("UNLOCKED" is displayed on cancellation. Disconnecting the power cable from power outlet does not cancel the lock.)
</p>
</ti3>
</ti2>
<ti2>
<ttl><html:a name="TITLE9_6">9.6 Service Precautions</html:a>
</ttl>
<ti3>
<ttl><html:a name="TITLE9_6_1">9.6.1 Recovery after the DVD player is repaired</html:a>
</ttl>
<ul>
<li>
<p>When the FLASH ROM IC or DVD Module P.C.B. is replaced, carry out the recovery processing to optimize the drive.
</p>
<p>Playback the recovery disk to process the recovery automatically.
</p>
</li>
<li>
<p>Recovery disc (Product number: RFKZD03R005) [SPG]
</p>
</li>
<li>
<p>Performing recovery process
</p>
<ol>
<li>
<p>Load the recovery disc RFKZD03R005 on to the player and run it.
</p>
</li>
<li>
<p>Recovery is performed automatically. When it is finished, a message appears on the screen.
</p>
</li>
<li>
<p>Remove the recovery disc.
</p>
</li>
<li>
<p>Turn off the power.
</p>
</li>
<li>
<p>Initialize the main unit.
</p>
</li>
</ol>
</li>
</ul>
</ti3>
<ti3>
<ttl><html:a name="TITLE9_6_2">9.6.2 Firmware version-up of the DVD player</html:a>
</ttl>
<ul>
<li>
<p>The firmware of the DVD player may be renewed to improve the quality including operability and playability to the substandard discs.processing to optimize the drive.
</p>
<p>The recovery disc has also firmware version-up.
</p>
</li>
<li>
<p>After version-up, recovery processing is executed automatically.
</p>
</li>
<li>
<p>Part number of the recovery disc for version-up will be noticed when it is supplied.
</p>
</li>
<li>
<p>Updating firmware
</p>
<ol>
<li>
<p>Load the recovery disc on to the player and run it.
</p>
</li>
<li>
<p>Firmware version of the player is automatically checked. Appropriate message appears whenever necessary.
</p>
</li>
<li>
<p>Using remote controller&#700;s cursor key, select whether version updating is to be done or not. (Selection of Yes&#47;No)
</p>
</li>
<li>
<p>a. If Yes is selected, version updating is performed.
</p>
<p>b. If No is selected, only recovery is performed.
</p>
</li>
<li>
<p>a. When updating is finished, remove the disc according to the message appearing on the screen.
</p>
<p>b. Remove the disc according to the message appearing on the screen.
</p>
</li>
<li>
<p>Turn off the power.
</p>
</li>
</ol>
</li>
</ul>
<topic>
<ttl>Note:
</ttl>
<p>If the AC power supply is shut out during version-up due to a power failure, the version-up is improperly carried out.
</p>
<p>In such a case, replace the FLASH ROM IC and carry out the version-up again.
</p>
</topic>
</ti3>
<ti3>
<ttl><html:a name="TITLE9_6_3">9.6.3 DVD Module P.C.B. Reset </html:a>
</ttl>
<ul>
<li>
<p>When after replacing FLASH ROM IC or DVD Module P.C.B., FL displays error code &#8220; DVD F897&#8221;. This means the unit is not initialized properly and the following process needs to be carry out.
</p>
</li>
<li>
<p>Procedures:
</p>
<ol>
<li>
<p>Press 
<graphic loc="graphic27" sizex="9.991mm" sizey="7.366mm"><html:img src="v9rem_10.png" border="0"></html:img>
</graphic> on remote control while pressing &#8220;STOP&#8221;  button on main unit. (To enter into initialization)
</p>
</li>
<li>
<p>FL display show &#8220;INIT&#8221;
</p>
</li>
<li>
<p>While still pressing &#8220;STOP&#8221; button on main unit, press &#8220;ENTER&#8221; on remote control. (To reset the unit)
</p>
</li>
<li>
<p>FL will display &#8220;RESET&#8221; before FL display will change to TOC reading again.
</p>
</li>
<li>
<p>Power off unit. Unplug the AC cord.
</p>
</li>
<li>
<p>Power on the unit. It should be no problem. If problem persist check on the DVD Module P.C.B. or FLASH ROM IC.
</p>
</li>
</ol>
</li>
</ul>
</ti3>
</ti2>
</other>
</html:body>
</svctechdoc>
