<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="MD0707029CE.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE11">11 Service Position</html:a>
</ttl>
<ti2>
<ttl><html:a name="TITLE11_1">11.1 Checking &#38; Repairing Main P.C.B.</html:a>
</ttl>
<p>
<emp>Step 1
</emp> Remove the top cabinet to service Main P.C.B.
</p>
<fig>
<graphic loc="graphic137" sizex="76.966mm" sizey="73.658mm"><html:img src="v9crmp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Main P.C.B can be checked at its original position.
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_2">11.2 Checking &#38; Repairing Speaker P.C.B.</html:a>
</ttl>
<p>
</p>
<p>
<emp>Step 1
</emp> Remove the top cabinet to service Speaker P.C.B.
</p>
<fig>
<graphic loc="graphic138" sizex="61.401mm" sizey="76.031mm"><html:img src="v9crspp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Speaker P.C.B can be checked at its original position.
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_3">11.3 Checking &#38; Repairing Panel P.C.B.</html:a>
</ttl>
<p>
<emp>Step 1
</emp> Remove the top cabinet.
</p>
<p>
<emp>Step 2
</emp> Remove 2 screws at the rear panel.
</p>
<p>
<emp>Step 3
</emp> Release the claws at each side the front panel.
</p>
<p>
<emp>Step 4
</emp> Detach the DVD&#47;CD changer mechanism unit in the direction of arrow.
</p>
<fig>
<graphic loc="graphic139" sizex="87.000mm" sizey="81.853mm"><html:img src="v9crpp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 5
</emp> Release the tab at each side of the front panel.
</p>
<p>
<emp>Step 6
</emp> Release the hooks at the bottom of the front panel.
</p>
<fig>
<graphic loc="graphic140" sizex="87.000mm" sizey="94.485mm"><html:img src="v9crpp2.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 7
</emp> Position the DVD&#47;CD changer mechanism unit according to the diagram shown.
</p>
<p>
<emp>Note : 
</emp>An object (eg. box) can be placed beneath the DVD&#47;CD changer mechanism unit to adjust its position height.
</p>
<p>
<emp>Step 8
</emp> Move one side of the front panel slightly forward to service Panel P.C.B.
</p>
<fig>
<graphic loc="graphic141" sizex="79.497mm" sizey="79.417mm"><html:img src="v9crpp3.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_4">11.4 Checking &#38; Repairing Deck P.C.B.</html:a>
</ttl>
<ul>
<li>
<p>Follow (Step 1) to (Step 7) of Item 11.3. 
</p>
</li>
</ul>
<p>
</p>
<p>
<emp>Step 1
</emp> Move one side of the front panel slightly forward.
</p>
<p>
<emp>Step 2
</emp> Remove 1 screw.
</p>
<p>
<emp>Step 3
</emp> Remove the deck shield plate.
</p>
<p>
<emp>Note : 
</emp>Deck P.C.B. can be checked at its original position.
</p>
<fig>
<graphic loc="graphic142" sizex="84.750mm" sizey="78.866mm"><html:img src="v9crdp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>An object (eg. box) can be placed beneath the DVD&#47;CD changer mechanism unit to adjust its position height.
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_5">11.5 Checking &#38; Repairing Deck Mechanism P.C.B.</html:a>
</ttl>
<ul>
<li>
<p>Follow (Step 1) to (Step 7) of Item 11.3. 
</p>
</li>
</ul>
<p>
</p>
<p>
<emp>Step 1
</emp> Move one side of the front panel slightly forward to check Deck Mechanism P.C.B .
</p>
<fig>
<graphic loc="graphic143" sizex="77.953mm" sizey="73.660mm"><html:img src="v9crdem1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>An object (eg. box) can be placed beneath the DVD&#47;CD changer mechanism unit to adjust its position height.
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_6">11.6 Checking &#38; Repairing Mic P.C.B.</html:a>
</ttl>
<ul>
<li>
<p>Follow (Step 1) to (Step 7) of Item 11.3. 
</p>
</li>
</ul>
<p>
</p>
<p>
<emp>Step 1
</emp> Move one side of the front panel slightly forward to remove the washer head screw from Mic P.C.B .
</p>
<fig>
<graphic loc="graphic144" sizex="87.000mm" sizey="76.675mm"><html:img src="v9crmip1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 2
</emp> Position Mic P.C.B according to the diagram shown.
</p>
<p>
<emp>Note : 
</emp>An object (eg. box) can be placed beneath the DVD&#47;CD changer mechanism unit to adjust its position height.
</p>
<fig>
<graphic loc="graphic145" sizex="67.784mm" sizey="65.500mm"><html:img src="v9crmip2.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Insulate Mic P.C.B from other parts with insulating material (eg. plastic).
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_7">11.7 Checking &#38; Repairing DVD Module P.C.B.</html:a>
</ttl>
<caution>
<ttl>Important notes: Ensure all the trays are in the &#8220;STOCK&#8221; position before proceeding to the disassembly of the traverse unit. For procedures to set the trays in &#8220;STOCK&#8221; position, please refer to original
Service Manual for CRS1D, Section 4.3. Setting the trays in &#8220;STOCK&#8221; position,  Order No. MD0603065A3.</ttl>
</caution>
<p>
</p>
<ul>
<li>
<p>Follow (Step 1) to (Step 7) of Item 11.3. 
</p>
</li>
</ul>
<p>
</p>
<ul>
<li>
<p>Disassembly of Side A of DVD Module P.C.B. 
</p>
</li>
</ul>
<p>
<emp>Step 1
</emp> Flip over the DVD&#47;CD changer mechanism unit and position it according to the diagram shown to service side A of DVD Module P.C.B.
</p>
<fig>
<graphic loc="graphic146" sizex="71.882mm" sizey="70.273mm"><html:img src="v9crdmp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Side A of DVD Module P.C.B can be checked at its original position.
</p>
<p>
</p>
<ul>
<li>
<p>Disassembly of Side B of DVD Module P.C.B. 
</p>
</li>
</ul>
<p>
<emp>Step 2
</emp> Remove 4 screws from DVD Module P.C.B.
</p>
<fig>
<graphic loc="graphic147" sizex="87.000mm" sizey="86.581mm"><html:img src="v9crdmp2.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 3
</emp> Flip over DVD Module P.C.B. to the side B and position it according to the diagram shown. 
</p>
<fig>
<graphic loc="graphic148" sizex="87.000mm" sizey="81.643mm"><html:img src="v9crdmp3.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>An object (eg. box) can be placed beneath the DVD&#47;CD changer mechanism unit to adjust its position height.
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_8">11.8 Checking &#38; Repairing D-Amp P.C.B.</html:a>
</ttl>
<p>
<emp>Step 1
</emp> Remove the top cabinet.
</p>
<p>
<emp>Step 2
</emp> Remove the DVD&#47;CD changer mechanism unit.
</p>
<p>
<emp>Step 3
</emp> Remove Main P.C.B.
</p>
<p>
<emp>Step 4
</emp> Remove 3 screws from the D-Amp P.C.B.
</p>
<p>
<emp>Step 5
</emp> Remove 2 screws from the SMPS P.C.B.
</p>
<fig>
<graphic loc="graphic149" sizex="71.323mm" sizey="80.500mm"><html:img src="v9crdap1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 6
</emp> Remove 1 screw at the rear panel.
</p>
<p>
<emp>Step 7
</emp>  Release the tab at each side of the rear panel in the direction of arrow.
</p>
<fig>
<graphic loc="graphic150" sizex="87.000mm" sizey="73.811mm"><html:img src="v9crdap2.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 8
</emp> Release the tab at each side of the front panel in the direction of arrow.
</p>
<p>
<emp>Step 9
</emp> Release the 2 hooks at the bottom part of the front panel.
</p>
<p>
<emp>Step 10
</emp> Remove the bottom chassis.
</p>
<fig>
<graphic loc="graphic151" sizex="87.000mm" sizey="93.873mm"><html:img src="v9crdap3.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 11
</emp> Flip the unit (including the front panel, rear panel, D-Amp P.C.B., SMPS P.C.B. &#38; Speaker P.C.B.) vertically and position it according to the diagram shown.
</p>
<fig>
<graphic loc="graphic152" sizex="84.836mm" sizey="79.851mm"><html:img src="v9crdap4.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 12
</emp> Connect Main P.C.B at the connectors (CN2810 &#38; CN5603) on D-Amp P.C.B and (CN5902) on SMPS P.C.B.
</p>
<p>
<emp>Step 13 
</emp>Connect cables at the connectors (CN2602, CNP2101, CNP2601, CNP2913 &#38; W1A) on Main P.C.B.
</p>
<fig>
<graphic loc="graphic153" sizex="87.000mm" sizey="83.143mm"><html:img src="v9crdap5.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 14 
</emp>Connect DVD&#47;CD changer mechanism unit at the connectors (CN2036 &#38; CN2038) on Main P.C.B.
</p>
<p>
<emp>Step 15 
</emp>Connect the grounding wires to the connectors (CNP2032 &#38; CNP2034) on Main P.C.B.
</p>
<fig>
<graphic loc="graphic154" sizex="86.276mm" sizey="74.507mm"><html:img src="v9crdap6.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Step 16 
</emp>Position D-Amp P.C.B according to the diagram shown.
</p>
<fig>
<graphic loc="graphic155" sizex="66.820mm" sizey="73.953mm"><html:img src="v9crdap8.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Insulate D-Amp P.C.B from other parts with insulating material (eg.plastic).
</p>
</ti2>
<ti2>
<ttl><html:a name="TITLE11_9">11.9 Checking &#38; Repairing SMPS P.C.B.</html:a>
</ttl>
<ul>
<li>
<p>Follow (Step 1) to (Step 15) of Item 11.8. 
</p>
</li>
</ul>
<p>
</p>
<p>
<emp>Step 1 
</emp>Position SMPS P.C.B according to the diagram shown.
</p>
<fig>
<graphic loc="graphic156" sizex="66.109mm" sizey="76.844mm"><html:img src="v9crsmp1.png" border="0"></html:img>
</graphic>
</fig>
<p>
<emp>Note : 
</emp>Insulate SMPS P.C.B from other parts with insulating material (eg.plastic).
</p>
</ti2>
</other>
</html:body>
</svctechdoc>
