<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="MD0707029CE.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE3">3 Precaution of Laser Diode</html:a>
</ttl>
<fig>
<graphic loc="graphic6" sizex="180.000mm" sizey="22.521mm"><html:img src="v9pld1.png" border="0"></html:img>
</graphic>
</fig>
<caution>
<ttl id="afdffssd">
</ttl>
<p>This product utilizes a laser diode with the unit turned on, invisible laser radiation is emitted from the pickup lens.
</p>
<p>Wavelength : 662nm (DVD)&#47;785nm (CD)
</p>
<p>Maximum output radiation power from pickup : 100&#181;W&#47;VDE 
</p>
<p>Laser radiation from pickup unit is safety level, but be sure the followings: 
</p>
<ol>
<li>
<p>Do not disassemble the pickup unit, since radiation from exposed laser diode is dangerous. 
</p>
</li>
<li>
<p>Do not adjust the variable resistor on the pickup unit. It was already adjusted.
</p>
</li>
<li>
<p>Do not look at the focus lens using optical instruments.
</p>
</li>
<li>
<p>Recommend not to look at pickup lens for a long time.
</p>
</li>
</ol>
</caution>
<fig>
<graphic loc="graphic7" sizex="118.110mm" sizey="142.325mm"><html:img src="v9pld2.png" border="0"></html:img>
</graphic>
</fig>
</other>
</html:body>
</svctechdoc>
